# Requirements:

BellWin USB Power Splitter connected to Host via USB

# Script usage:

python usb\_pdu.py <outlet#> <command>

**Note:** Script assumes that there is only one BellWin USB Power Splitter connected to the host

# examples:

**Turn off outlet 1**

python usb\_pdu.py 1 OFF

**Turn on outlet 1**

python usb\_pdu.py 1 ON

**Cycle outlet 1**

python usb\_pdu.py 1 Cycle